High Performance Oxygen Analyzer

CGM-9100 Series

지르코니아식 산소분석기

주요 명세 • Measuring parameter : oxygen concentration • Measuring medium : gaseous atmosphere • Measuring principle : Zirconia (ZrO2) type sensor • Measuring ranges : 0.1~20.9 % O2 • Output - signal : DC 4 ~ 20 mA, 2-Wires • Accuracy : ± 0.5% of measuring range • Response time(T90) : 2 to 10sec. • Power voltage : AC110/220V 60Hz • Warm up time : approx. 10 min. • Calibration : Auto zero, Span • ambient temperature : In air ~ 650℃	특 징 각종 열설비에서 연소효율을 극대화시키거나, 노(爐)내의 분위기조절을 위하여 산소농도를 측정하는 지르코니아식 산소분석기 • 직접삽입식으로 샘플링 불필요 • 응답속도가 빠르고 정확하며 연속측정가능 • 일정한 센서온도유지로 저온부식방지 • 고성능 ZrO2 방식 채택 • 제철소, 가스시설물, 화학공장, 정유공장, 식품공장 반도체공장, N2 솔더링머신 등에 적합 • 예고 없이 모양이 바뀔 수 있음.

	checkwin #152-12, Galsan-dong, Bupyung-ku Inchon, 403-080, Korea TEL:82-32-514-0993 FAX:82-32-514-0994 www.checkwin.co.kr

COMPONENT

1.CGM-9100-M

1.Monitor

Power:220VAC 60Hz,60Watt

Measuring ranges : 0.1~20.9 % O2

Output - signal : DC 4 ~ 20 mA

2.Sensor

Material: ZR2O3 + Platinum

Output signal: approx 120 mv ~ 0 mv

(0.1~20.9 % O2)

with TC, "k" type

3.Probe

Material: STS 304

Power:220VAC 60Hz,500Watt

Length(mm):350,500,1000

2.CGM-9000-S

3.CGM-9000-P

	checkwin #152-12, Galsan-dong, Bupyung-ku Inchon, 403-080, Korea TEL:82-32-514-0993 FAX:82-32-514-0994 www.checkwin.co.kr