Portable & Panel mount Oxygen Analyzer

EGA-2000 Series

산소분석기

주요 명세 • Measuring parameter : oxygen concentration • Measuring medium : gaseous sampling • Measuring principle : limiting current type sensor • Measuring ranges : 1 ~ 1000 ppm O2 , 1 ~ 10000 ppm O2 0.01 ~ 2.0 % O2 , 0.01 ~ 5.0% O2 0.01 ~ 25.0 % O2 , 0.1 ~ 99.0 % O2 • Output - signal : DC 4 ~ 20 mA, RS-485 • Accuracy : 1% of measuring range • Response time(T90) : 2 to 10sec. • Operating Temperature : -10 ~ +50 • Operating Humidity : 0 ~ 95%RH • Sampling Connection : 1/4" Tube • Power voltage : AC220V 60Hz • Warm up time : approx. 3 min. • Alarm : AL1, AL2, Fault • Alarm Contact : Relay Contact • Flow rate : 500 ml/min • Pressure : 0.5 kg/㎠ • Demension : 250(W) x 132.5(H) x 250(D)mm	특 징 • 첨단 기능의 휴대형/판넬 매입형 가스 모니터링 • 고성능 마이크로프로세서 탑재에 의한 정확도 및 편리성 증대 • 예비경보와 주 경보의 2단계 경보 설정 • 순간적인 이상신호를 제거하는 경보지연 시간설정 • 자기진단 기능 및 소프트웨어방식의 교정기능 보유 • RS-485 통신기능 보유 • 제철소, 가스시설물, 화학공장, 정유공장, 식품공장 반도체공장, N2 솔더링머신 등에 적합

	CHECKWIN 152-12, Galsan-dong, Bupyung-ku Inchon, 403-080, Korea TEL:82-32-514-0993 FAX:82-32-514-0994 www.checkwin.co.kr, www.checkwin.kr